## Engine Lubrication

#### Oil Pump Overhaul

8-9

Exploded View

1. DOWEL PIN
2. INNER ROTOR
3. PUMP COVER
4. OUTER ROTOR
5. O-RING

   Replace

6. PUMP HOUSING

   Apply liquid gasket to mating surface of the cylinder block when installing

7. RELIEF VALVE

   Valve must slide freely in housing bore.

   Replace if scored.

8. SEALING BOLT

   39 Nm (4.0 kgf/m, 29 lbf/ft)

9. SPRING
10. OIL SEAL

    Replace