## Cylinder Head

#### Rocker Arms and Shafts Disassembly/Reassembly

6-35

NOTE:

- Identify parts as they are removed to ensure reinstallation in original location.
- Inspect the rocker shafts and rocker arms (see page 6-38).
- The rocker arms must be installed in the same positions if reused.
- When removing or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders, springs and rocker arms on the shaft.
- Prior to reassembling, clean all the parts in solvent, dry them and apply lubricant to any contact points.

D15Y4, D16V2, D16W7, D17A2, D17A5, D17Z3 engines:

1. RUBBER BAND
2. INTAKE ROCKER SHAFT
3. COLLAR B
4. INTAKE ROCKER ARM ASSEMBLY
5. COLLAR A
6. No. 1 CAMSHAFT HOLDER
7. EXHAUST ROCKER ARM A
8. Letter "A" is stamped on the rocker arm.
9. EXHAUST ROCKER SHAFT
10. Letter "B" is stamped on the rocker arm.
11. SPRING
12. EXHAUST ROCKER ARM B
13. No. 5 CAMSHAFT HOLDER
14. No. 4 CAMSHAFT HOLDER
15. No. 3 CAMSHAFT HOLDER
16. No. 2 CAMSHAFT HOLDER