## Engine Assembly

#### Engine Removal (cont'd)

5-5

1. Remove the harness clamps (A) and grommet (B), then pull the engine wire harness through the bulkhead.

LHD models:

RHD models:

1. Relieve fuel pressure (see page 11-115).

1. Remove the fuel feed hose (see page 11-120).

1. Remove the Evaporative Emission (EVAP) canister hose (A) and brake booster vacuum hose (B).

1. Remove the clutch slave cylinder (A) and clutch line bracket mounting bolt (B).

a a a