## Sunroof

#### Position Switch Adjustment

20-61

1. Remove the headliner (see page 20-68).
2. With the sunroof wrench, close the glass (A) fully:

- Make sure both link lifters (B) are parallel, and in the position shown.
- Check the glass fit to the roof panel and the glass height (see page 20-52).

3. With an open-end wrench, loosen the position switch mounting bolts (C).
4. Adjust the position switch (D):

- Move the switch plate (E) a little at a time, then secure it at the position where you hear a faint click when the switch cam (F) pushes the position switch (open/close).
- Check that the switch plate contacts the switch bracket (F).

5. Check the operation of the glass (from the tilt-up position to fully closed position, from the fully open position to the fully closed position) by operating the sunroof switch.