## Front Side Frame/Outrigger

#### Removal (cont'd)

3-45

- Check the side frame bulkhead rear for position and damage. If Necessary replace it.

  1. SUB-FRAME REAR BRACKET
  2. SIDE FRAME BULKHEAD REAR
  3. SIDE FRAME EXTENSION

- If necessary, replace the side frame extension rear, outrigger and sub-frame rear bracket as an assembly.

NOTE: When removing the outrigger, leave the inside sill extension attached to the inside sill, if possible.

Passenger compartment side:

1. OUTRIGGER
2. SUB-FRAME REAR BRACKET
3. SIDE FRAME EXTENSION REAR
4. OUTRIGGER
5. INSIDE SILL EXTENSION
6. FLOOR FRAME
7. SIDE FRAME EXTENSION REAR
8. SUB-FRAME REAR BRACKET