## Clutch

#### Clutch Master Cylinder Overhaul

12-6

Exploded View

1. CLUTCH MASTER CYLINDER SEAL
2. MASTER CYLINDER BODY

   Check the cylinder wall for scoring and wear.

3. RESERVOIR HOSE

   Inspect for damage, leaks, interference and twisting.

4. RETAINING CLIP

   Replace.

5. RETAINING CLIP HOLDER

   (LHD type only)

6. RESERVOIR
7. (Brake Assembly Lube)
8. (Brake Assembly Lube)
9. PUSH ROD
10. CIRCLIP
11. LOCK PIN

    Replace.

12. YOKE
13. PEDAL PIN
14. STOPPER

    Check for damage and bending.

15. CLIP CATCHES ARE ON THE SIDE MARKED WITH A SMALL ARROW

12-5c 12-7 home