## Interior Trim

#### Trim Removal/Installation - Door Area

20-64

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.
- LHD is shown, RHD is symmetrical.

Remove the trim as shown:

- To remove the driver's kick panel (LHD), remove the footrest (see step 2 on page 20-70).
- To remove the seat side trim, remove the rear seat side bolster, folding type rear seat (see page 20-95), or the rear seat-back, fixed type rear seat (see page 20-96).
- To remove the front side cap and opener lock cylinder (for some models), refer to trunk lid opener/fuel fill door opener replacement (see page 20-129.

Install the trim in the reverse order of removal, and note these items:

- Replace any damaged clips.
- Apply liquid thread lock to the front seat belt upper anchor bolt before installation.
- Before installing the anchor bolts, make sure there are no twists or kinks in the belts.

  Fastener Locations
  A : Clip,2 (Black) | B : Clip, 3 (White) | C : Clip, 9 | D : Clip, 1 | E : Clip, 1
  1. FRONT SEAT BELT UPPER ANCHOR BOLT

     7/16-20 UNF

     32 Nm (3.3 kgf m, 24 lbf ft)

  2. CENTRE PILLAR UPPER TRIM
  3. FRONT DOOR OPENING TRIM
  4. FRONT PILLAR TRIM
  5. KICK PANEL
  6. UPPER ANCHOR COVER
  7. OPENER LOCK CYLINDER

     (For some models)

  8. FRONT SIDE CAP
  9. FRONT DOOR SILL TRIM
  10. FRONT SEAT BELT LOWER ANCHOR BOLT

      7/16-20UNF

      32 Nm (3.3 kgf m, 24 lbf ft)

  11. SEAT SIDE TRIM
  12. REAR PILLAR TRIM
  13. CENTRE PILLAR LOWER PROTECTOR
  14. CENTRE PILLAR LOWER TRIM
  15. REAR DOOR OPENING TRIM