## Wiper/Washers

#### Headlight Washer Control Unit Input Test

22-176

KG model

1. Remove the dashboard lower cover.
2. Disconnect the 9P connector (A) from the headlight washer control unit (B).

3. Inspect the connector and socket terminals to be sure they are all making good contact.

- If the terminals are bent, loose or corroded, repair them as necessary and recheck the system.
- If the terminals look OK, go to step 4.