## Engine Assembly

#### Engine Installation (cont'd)

5-18

24. Install the A/C compressor (A), then install the alternator lower bracket (B).

25. Install the A/C hose bracket (A) and P/S hose bracket (B).

26. Loosely install the alternator.
27. Adjust the alternator belt tension (see page 4-38) or the alternator-compressor belt tension (see page 4-37).
28. Loosely install the P/S pump belt and pump.
29. Adjust the P/S pump belt (see page 17-23).
30. Push the ECM/PCM connectors through the bulkhead, then install the grommet (A).

RHD models:

LHD models:

31. Install the harness clamps (B).