## Cruise Control

#### Actuator Cable Adjustment

4-49
Clutch Pedal Position Switch Test

1. Check that the actuator cable (A) moves smoothly with no binding or sticking.

2. Measure the amount of movement of the output linkage (B) until the engine speed starts to increase. At first, the output linkage should be located at the fully closed position (C). The free play (D) should be 3.75 + 0.5 mm (0.15 +0.02 in.).
3. If the free play is not within specs, loosen the locknut, and turn the adjusting nut until the free play is as specified, then retighten the locknut.

1. Disconnect the 2P connector from the clutch pedal position switch (A).

CLUTCH PEDAL POSITION SWITCH 2P CONNECTOR

2. Remove the clutch pedal position switch.
3. Check for continuity between the terminals according to the table.

4. If necessary, replace the clutch pedal position switch or adjust the pedal height (see page 12-4).