## Honda Multi Matic Transmission/CVT

#### Transmission Removal (cont'd)

14-328

26. Make the appropriate reference lines at positions A and B that line up with the centre of the sub-frame mounting bolts (C).

27. Support the sub-frame with a 4 x 4 x 40 in. piece of wood and a jack.

28. Remove the 10 x 1.25 mm bolts (A) and four sub-frame mounting bolts (B), then lower the sub-frame (C).

29. Remove the driveshafts from the differential. Coat all precision finished surfaces with clean engine oil, then tie plastic bags over the driveshaft ends.