## Cylinder Head

#### Cylinder Head Removal (cont'd)

6-16

1. Remove the injector seals from top of the cylinder head cover (A) and side of the cylinder head cover (B).

1. Remove the cylinder head cover.

1. Remove the bolts (A) from the dust cover.

1. Loosen bolts (A).

1. Loosen bolts; bracket fixing (B).

1. Loosen bolt; bracket fixing (C).

1. Remove bracket (D).

1. Remove retainer; injector (E).

1. Remove injector assembly (F).

a a a