## Fuel and Emissions Systems

#### System Descriptions (cont'd)

11-22

Vacuum Hose Routing (cont'd)

1. CLAMP TO HARNESS
2. HARNESS; P/P
3. EVRV
4. EGR VALVE
5. INSERTION LENGTH IS MORE THAN 15mm
6. VSS
7. MUST INSERT TO THE END.
8. ASSEMBLE TO 3WAY.
9. INSERTION LENGTH IS MORE THAN 10mm.
10. 4WAY
11. ASSEMBLE TO EVRV.
12. MUST INSERT TO THE END.
13. 3WAY
14. EVRV

No. | Part Name | QTY | Remarks
(8) | HOSE; VACUUM, EGR V-EVRV | 1 | ø10
(10) | HOSE; VACUUM, TURBO-3WAY | 1 | ø10
(11) | HOSE; VACUUM, EGR-3WAY | 1 | ø10
(12) | HOSE; VACUUM, 3WAY-A/C | 1 | ø10
(14) | CLIP; HOSE, VACUUM | 2 | ø7-ø10
(18) | CLIP; HOSE, VACUUM | 1 | ø10-ø10

a a a