## Dashboard

#### Steering Hanger Beam Replacement (cont'd)

20-227

6. Remove the bolts (A) and screws (B) securing the dashboard (C) and steering hanger beam (D) and disconnect the power mirror switch connector (E). On auto A/C model, disconnect the in-car temperature sensor connector (F). Separate the dashboard and steering hanger beam.

Fastener Locations
A : Bolt, 4 | B : Screw. 8

7. Install the beam in the reverse order of removal and note these items:

- Make sure the dashboard wire harness (G) is not pinched.
- Make sure the connectors are connected properly.