## Fuel Supply System

#### Fuel Tube/Quick-Connect Fittings Installation (cont'd)

11-137

4. Align the quick-connect fittings with the pipe (A), and align the retainer (B) locking pawls with the connector (C) grooves. Then press the quick-connect fittings onto the pipe until both retainer pawls lock with a clicking sound.

NOTE: If it is hard to connect, put a small amount of new engine oil on the pipe end.

Connection with new retainer:

Reconnection to existing retainer:

5. Make sure the connection is secure and that the pawls are firmly locked into place; check visually and by pulling the connector.

6. Reconnect the negative cable to the battery, and turn the ignition switch ON (II). The fuel pump will run for about 2 seconds, and fuel pressure will rise. Repeat 2 or 3 times, and check that there is no leakage in the fuel supply system.