## SRS

#### DTC Troubleshooting (cont'd)

23-86

DTC 13-1, 13-2: Internal Failure of the Driver's Side Impact Sensor (With OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Replace the driver's side impact sensor (see page 23-177).

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

DTC 14-1, 14-2: Internal Failure of the Front Passenger's Side Impact Sensor (With OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Replace the front passenger's side impact sensor (see page 23-177).

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).