## Frame

#### Frame Repair Chart

20-48

Top View

Unit : mm (in) | a | For sub-frame Ø15 (0.59) | i | For sub-frame Ø11 (0.43)
Ø: Inner diameter | b | For engine mount Ø13 (0.51) | j | For damper mount Ø11.5 (0.45)
| c | For engine mount Ø13 (0.51) | k | For damper mount Ø11.5 (0.45)
| d | For engine mount Ø13 (0.51) | l | Damper centre Ø78 (3.07)
| e | For transmission mount Ø13 (0.51) | m | For sub-frame Ø15 (0.59)
| f | For transmission mount Ø13 (0.51) | n | Locating hole Ø25 (0.98)
| g | For transmission mount Ø13 (0.51) | o | Locating hole Ø50 (1.97)
| h | For damper mount Ø11.5 (0.45) |  |