## Front Suspension

#### Knuckle/Hub/Wheel Bearing Replacement

18-3

Exploded View

1. WHEEL BEARING, Replace.
2. SNAP RING
3. 5 mm SCREW

   5.9 Nm (0.6 kgf/m, 4.3 lbf/ft)

4. FLAT SCREW

   6 x 1.0 mm

   9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

5. SPINDLE NUT, Replace.

   24 x 1.5 mm

   245 Nm (25.0 kgf/m, 181 lbf/ft)

6. BRAKE DISC
7. HUB

   Check for deformation, damage and cracks.

8. SPLASH GUARD

   Check for corrosion, deformation and damage.

   Replace if rusted.

9. KNUCKLE

   Check for deformation and damage.

a a a