## Transmission Lower Valve Body

#### Lower Valve Body Assembly, ATF Strainer and ATF Pan Installation

14-384

1. Install the solenoid harness connector (A) with the new O-ring (B) (one bolt) and install the lower valve body assembly (C) with three ATF feed pipes (D) (eight bolts).

2. Install the ATF strainer (E) with the new O-ring (F) (two bolts).

3. Install the ATF pan (A) with the two dowel pins (B) and new ATF pan gasket (C) (14 bolts).

4. Install the breather cap (A) on the breather pipe (B) so its arrow points to the flywheel housing.