## Cylinder Head

#### Cylinder Head Cover Installation (cont'd)

6-56

7. Tighten the bolts in 2 or 3 steps. In the final step, tighten all bolts, in sequence, to 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft).

8. Install the harness holder (A) and throttle cable clamps (B).

9. Install the ignition coils (see page 4-24).
10. Check that all tubes, hoses and connectors are installed correctly.
11. After assembly, wait at least 30 minutes before filling the engine with oil.