## M/T Differential

#### Differential Thrust Clearance Adjustment

13-54

Special Tool Required Driver, 40 mm I.D. 07746-0030100

1. Install the 80 mm shim that's the same size as the one you removed.

2. Install the differential assembly into the clutch housing.

3. Install the transmission housing onto the clutch housing, then tighten the 8 mm flange bolts in a crisscross pattern in several steps.

8 x 1.25 mm

27 Nm (2.8 kgf/m, 20 Ibf/ft)

4. Use the special tool to bottom the differential assembly in the clutch housing.

5. Measure clearance between 80 mm shim and bearing outer race in transmission housing.

   Standard: | 0 - 0.10 mm (0 - 0.004 in.)