## Transmission Housing/Flywheel Housing

#### Secondary Gear Shaft Transmission Housing Bearing Replacement

14-360

Secondary Gear Shaft Flywheel Housing Bearing Replacement

Special Tools Required

- Adjustable bearing remover set, 07JAC-PH80000
- Handle driver, 07749-0010000
- Driver attachment, 72 x 75 mm, 07746-0010600

1. Remove the secondary gear shaft bearing (A) from the transmission housing (B) with the special tool.

2. Install the new secondary gear shaft bearing until it bottoms in the transmission housing with the special tools.

Special Tools Required

- Adjustable bearing remover set, 07JAC-PH80000
- Handle driver, 07749-0010000
- Driver attachment, 62 x 68 mm, 07746-0010500

1. Remove the secondary gear shaft bearing (A) from the flywheel housing (B) with the special tool.

2. Install the new secondary gear shaft bearing until it bottoms in the flywheel housing with the special tools.