## Shafts and Clutches

#### Countershaft 4th Gear Clearance Inspection (cont'd)

14-199

6. Tighten the locknut (G) to 29 Nm (3.0 kgf/m, 22 lbf/ft). The locknut has left-hand threads.

7. Measure the clearance between the 2nd gear (A) and 28 mm distance collar (B) with a feeler gauge (C) in at least 3 places. Use the average as the actual clearance.

   STANDARD: 0.10-0.18 mm (0.004-0.007 in.)

8. If the clearance is out of standard, disassemble the countershaft. Remove the 28 mm distance collar and measure its length.

9. Select and install a new distance collar, assemble the countershaft, then recheck.

   DISTANCE COLLAR, 28 mm

   No. | Part Number | Thickness
   1 | 90503-PC9-000 | 39.00 mm (1.535 in.)
   2 | 90504-PC9-000 | 39.10 mm (1.539 in.)
   3 | 90505-PC9-000 | 39.20 mm (1.543 in.)
   4 | 90507-PC9-000 | 39.30 mm (1.547 in.)
   5 | 90508-PC9-000 | 39.05 mm (1.537 in.)
   6 | 90509-PC9-000 | 39.15 mm (1.541 in.)
   7 | 90510-PC9-000 | 39.25 mm (1.545 in.)
   8 | 90511-PC9-000 | 38.90 mm (1.531 in.)
   9 | 90512-PC9-000 | 38.95 mm (1.533 in.)

10. After replacing the distance collar, make sure the clearance is within standard.
11. Disassemble the shaft and gears.
12. Reinstall the bearing in the transmission housing (see page 14-177).