## Standards and Service Limits

#### Honda Multi Matic Transmission and HMM Differential

2-19

Item | Measurement | Qualification | Standard or New | Service Limit
HMM Transmission Fluid | Capacity | Use genuine Honda ATF-Z1 | For fluid change: 3.1 l (3.3 US qt, 2.7 Imp qt)
For overhaul: 5.6 l (5.9 US qt, 4.9 Imp qt)
Hydraulic pressure | Forward clutch pressure | At 1,500 rpm (min-1) in position | 1.4-1.75 MPa (14.3-17.8 kgf/cm2, 203-253 psi)
Reverse brake pressure | At 1,500 rpm (min-1) in position | 1.4-1.75 MPa (14.3-17.8 kgf/cm2, 203-253 psi)
Drive pulley pressure | At 1,500 rpm (min-1) in position | 0.2-0.7 MPa (2.0-7.1 kgf/cm2, 28-101 psi)
Driven pulley pressure | At 1,500 rpm (min-1) in position | 1.5-2.3 MPa (15.3-23.5 kgf/cm2, 218-334 psi)
Lubrication pressure | At 3,000 rpm (min-1) in position | Above 0.2 MPa (Above (0.2 kgf/cm2, 30 psi)
Torque converter | Stall speed Check with vehicle on level ground | D15Y4 engine in position | 2,500 rpm (min-1) | 2,350-2,650 rpm (min-1)
D15Y4 engine in , and positions | 3,000 rpm (min-1) | 2,800-3,100 rpm (min-1)
D17A2 engine in position | 2,500 rpm (min-1) | 2,350-2,650 rpm (min-1)
D17A2 engine in , and positions | 2,800 rpm (min-1) | 2,600-2,900 rpm (min-1)
ATF pump | ATF pump drive gear shaft O.D. |  | 9.98-9.99 mm (0.3929-0.3933 in.) | When worn or damaged
ATF pump driven gear shaft O.D. |  | 9.98-9.99 mm (0.3929-0.3933 in.) | When worn or damaged
ATF pump body bushing I.D. | Drive gear shaft | 10.0-10.015 mm (0.3937-0.3944 in.) | When worn or damaged
Driven gear shaft | 10.0-10.015 mm (0.3937-0.3944 in.) | When worn or damaged
ATF pump gear side clearance |  | 0.015-0.035 mm (0.0006-0.0014 in.) | -
ATF pump gear-to-body clearance | Drive gear | 0.035-0.0505 mm (0.0014-0.0020 in.) | -
| Driven gear | 0.035-0.0505 mm (0.0014-0.0020 in.) | -

" BORDER=0>