## Doors

#### Rear Door Hook Pin and Catch Replacement

20-24

Front and Rear Door Glass Adjustment

For Some Models

1. With a Torx T40 bit, remove the door hook pin (A) from the door.

2. With a Torx T40 bit, remove the bolts, then remove the door catch (A) from the body.

   Fastener Locations
   : Bolt, 2

3. Install the hook pin and catch in the reverse order of removal, and apply liquid thread lock to the threads of the door hook pin.

NOTE: Check the weatherstrips and glass run channel for damage or deterioration, and replace them if necessary.

1. Place the vehicle on a firm, level surface.
2. Remove these items:

- Door panel, front door (see page 20-7), rear door (see page 20-15)
- Plastic cover, front door (see page 20-3), rear door (see page 20-5)

3. Carefully move the glass (A) until you can see the glass mounting bolts (B), then loosen them.

   Front: