## PGM-FI System

#### DTC Troubleshooting (cont'd)

11-526

DTC 13: BARO Sensor Circuit Malfunction

1. Reset the ECM/PCM (see page 11-468).
2. Turn the ignition switch ON (II).

Is the MIL on and does it indicate DTC 13?

YES | - Substitute a known-good ECM/PCM and recheck. If symptom/indication goes away, replace the original ECM/PCM.
NO | - Intermittent failure, system is OK at this time (test-drive may be necessary).