## Engine Assembly

#### Engine Removal (cont'd)

5-4

1. Disconnect the harness connectors (A) and remove the harness clamp (B).

1. Remove the fuel feed hose (A) and fuel return hose (B).

1. Remove the lower panel, then disconnect the main wire harness connectors (A).

1. Remove the glove box stops and open the glove box.Disconnect the engine control module (ECM) connectors (B) and ground cable (C).

1. Remove the harness clamp (A) and disconnect the accelerator panel sensor connector (B).

a a a