## Opening Repair Chart

####

4-3

Unit: mm (in.)

Door and Windshield Openings:

1. A

   Windshield lower dashboard guide pin

2. B, C

   Windshield opening flange notch (2 places)

3. D, E, F, G

   Door opening flange notch (8 places)

Rear Window and Trunk Lid Openings:

1. H, I

   Rear window opening flange notch (3 places)

2. J

   Parcel shelf convex bead

3. K

   Trunk gutter area convex bead

4. L

   Rear gutter area outer panel flange end (2 places)

5. M

   Trunk seal flange water drain notch