## EPS Components

#### Steering Gearbox Overhaul

17-99

Exploded View

1. TORQUE SENSOR
2. MOTOR CONNECTOR
3. MOTOR
4. O-RINGS

   Replace.

5. PINION SHAFT GROMMET
6. GEARBOX HOUSING
7. STOP RING

   Replace.

8. LOCK SCREW

   162 Nm (16.5 kgf/m, 119 lbf/ft)

   Replace.

9. SLIDER GUIDE
10. RACK HOUSING
11. BOOT BAND

    Replace.

12. TIE-ROD END
13. TIE ROD

    54 Nm (5.5 kgf/m, 40 lbf/ft)

14. LOCK WASHER

    Replace.

15. BRACKET
16. O-RINGS

    Replace.

17. STOP PLATE

    Replace.

18. BOOT
19. BOOT BAND

    Replace.

20. LOCKNUT
21. RACK GUIDE SCREW
22. SPRING
23. DISC WASHER
24. RACK GUIDE