## EPS Components

#### System Description

17-70

EPS Control Unit Inputs and Outputs at Connector A (2P)

EPS CONTROL UNIT CONNECTOR A (2P)

Wire side of female terminals

Terminal number | Wire colour | Terminal sign (Terminal name) | Description | Measurement
Terminals | Conditions Ignition switch ON (II) | Voltage
1 | WHT/BLU | + BAT (Plus battery) | Power source for the actuator motor | 1-Ground | Every time | Battery voltage
2 | BLK | PG (Power ground) | Ground for the actuator motor | 2-Ground | - | -

EPS Control Unit Inputs and Outputs at Connector B (2P)

EPS CONTROL UNIT CONNECTOR B (2P)

Wire side of female terminals

Terminal number | Wire colour | Terminal sign (Terminal name) | Description | Measurement
Terminals | Conditions Ignition switch ON (II) | Voltage
1 | RED | M1 (Motor 1) | Drives the actuator motor | 1-Ground | - | -
2 | GRN | M2 (Motor 2) | Drives the actuator motor | 2-Ground | - | -