## Cylinder Head

#### Cylinder Head Removal (cont'd)

6-31

15. Remove the engine wire harness connectors and wire harness clamps from the intake manifold.

- Idle air control (IAC) valve connector
- Throttle position sensor connector
- Manifold absolute pressure (MAP) sensor connector
- Evaporative emission (EVAP) canister purge valve connector (Except KT, KW models)
- Engine coolant temperature (ECT) sensor connector
- Radiator fan switch connector
- CKP sensor connector
- TDC sensor connector
- Exhaust gas recirculation (EGR) connector (D14Z5, D15Y4, D16W7, D17A2 engines)
- VTEC solenoid valve connector (D15Y4, D16V2, D16W7, D17A2, D17A5, D17Z3 engines)
- VTEC oil pressure switch connector (D16W7 engine)
- Oil pressure sensor connector

16. Support the engine with a jack and wood block under the oil pan.
17. Remove the upper bracket.

18. Remove the cover (A), then remove the exhaust manifold (B).

D15Y5, D15Y6, D17A1, D17Z1, D17Z2 engines:

Except D15Y5, D15Y6, D17A1, D17Z1, D17Z2 engines: