## Side Sill Outer Panel

#### Removal

3-20

- Cut and pry off the side sill outer panel.
- Check the centre pillar stiffener and side sill reinforcement position and for damage and if necessary replace them.
- When removing the centre pillar stiffener, do not cut the centre pillar stiffener reinforcement; the centre pillar stiffener reinforcement is part of the centre pillar stiffener.
- When replacing the center pillar stiffener, remove the centre pillar separator, and glue the insulator at the separator mounted position.

  1. Outer panel cut line.
  2. Centre pillar stiffener cut line.
  3. CENTRE INNER PILLAR
  4. SIDE SILL REINFORCEMENT
  5. VIEW (Z)
  6. INSIDE SILL
  7. CENTRE PILLAR SEPARATOR
  8. SIDE SILL REINFORCEMENT
  9. OUTER PANEL
  10. CENTRE PILLAR STIFFENER
  11. CENTRE PILLAR STIFFENER REINFORCEMENT