## Engine Assembly

#### Engine Removal (cont'd)

5-6

15. Remove the harness clamps (A) and grommet (B), then pull the engine wire harness through the bulkhead.

RHD models:

LHD models:

16. Remove the throttle cable (A) by loosening the locknut (B), then slipping the cable end out of the accelerator linkage. Take care not to bend the cable when removing it. Always replace any kinked cable with a new one.

17. Remove the alternator, refer to the '01 Civic Shop Manual on this CD (see page 4-31).
18. Remove the air conditioning (A/C) hose bracket.