## Standards and Service Limits

#### Clutch

2-6

Item | Measurement | Qualification | Standard or New | Service Limit
Clutch pedal | Height from the floor |  | 197 mm (7.76 in.) | -
Stroke |  | 130-140 mm (5.1-5.5 in.) | -
Play |  | 10-16 mm (0.39-0.63 in.) | -
Disengagement height from the floor |  | 115 mm (4.53 in.) min. | -
Flyweel | Runout on clutch mating surface |  | 0.05 mm (0.002 in.) max. | 0.15 mm (0.006 in.)
Clutch disc | Rivet head depth |  | 1.65-2.25 mm (0.065-0.089 in.) min. | 0.7 mm (0.03 in.)
Thickness |  | 8.3-8.9 mm (0.33-0.35 in.) | 6.0 mm (0.24 in.)
Pressure plate | Warpage |  | 0.03 mm (0.001 in.) max. | 0.15 mm (0.001 in.)
Height if diaphragm spring fingers | Measured with special tool and feeler gauge | 0.6 mm (0.02 in.) max. | 0.8 mm (0.03 in.)

a a a