## Maintenance Schedule

#### Normal Conditions

3-4

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule (see page 3-6) do not apply.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120 | 135 | 150 | 165
miles x 1,000 | 9 | 18 | 27 | 36 | 45 | 54 | 63 | 72 | 81 | 90 | 99
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132
Replace engine oil |  |  |  |  |  |  |  |  |  |  |
Replace engine oil filter |  |  |  |  |  |  |  |  |  |  |
Replace air cleaner element |  |  |  |  |  |  |  |  |  |  |
Inspect valve clearance |  |  |  |  |  |  |  |  |  |  |
Replace fuel filter |  |  |  |  |  |  |  |  |  |  |
Drain fuel filter (water) |  |  |  |  |  |  |  |  |  |  |
Replace timing belt |  |  |  |  |  |  |  |  |  |  |
Inspect and replace drive belts | Inspect every 30,000 km (18,000 miles) or 2 years, replace every 150,000 km (90,000 miles) or 10 years
Replace engine coolant |  |  |  |  |  |  |  |  |  |  |
Replace transmission fluid |  |  |  |  |  |  |  |  |  |  |
Inspect front and rear brakes |  |  |  |  |  |  |  |  |  |  |
Replace brake fluid | Every 3 years
Check parking brake adjustment |  |  |  |  |  |  |  |  |  |  |
Replace pollen filter | Every 30,000 km (18,000 miles) or 1 year
Check lights alignment |  |  |  |  |  |  |  |  |  |  |
Test drive (noise, stability, dashboard operations) |  |  |  |  |  |  |  |  |  |  |
Visually inspect the following items:
Tie rod ends, steering gearbox and boots |  |  |  |  |  |  |  |  |  |  |
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS)
All fluid levels and condition of fluid
Exhaust system
Fuel lines and connections
Tyre condition

a a a