## Interior Trim

#### Trim Removal/Installation - Trunk Floor Area

20-31

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown.

Install the trim in the reverse order of removal, and note these items:

- Replace any damaged clips.
- Make sure the trunk compartment light connector is plugged in properly.

Fastener Locations

A : Clip, 3 B : Clip, 4 C : Clip, 2

(White)

1. TRUNK FLOOR MAT

   (With spare tyre)

2. HOOK
3. TRUCK FLOOR MAT
4. SPARE TYRE LID
5. HOLE
6. TRUNK FLOOR MAT

   (With normal tyre)

7. SPARE TYRE LID
8. RIGHT TRUNK SIDE FRONT SPACER

   (With normal tyre)

9. RIGHT TRUNK SIDE REAR SPACER

   (With normal tyre)

10. REAR SIDE TRIM PANEL
11. To rear side trim panel.
12. REAR TRIM PANEL
13. HOOK
14. To rear side trim panel.
15. To rear side trim panel.
16. LEFT TRUCK SIDE REAR SPACER

    (With normal tyre)

17. LEFT TRUNK SIDE FRONT SPACER

    (With normal tyre)

18. REAR SEAT-BACK COVER

a a a