## Fuel Supply System

#### Fuel Filter Replacement

11-296

1. The fuel filter should be replaced whenever the fuel pressure drops below the specified value (270-320 kPa, 2.8-3.3 kgf/cm2, 40-47 psi) after making sure that the fuel pump and the fuel pressure regulator are OK.
2. Relieve fuel pressure (see page 11-130).
3. Disconnect the hose and quick-connect fittings (A) (see page 11-293).

3. Remove the fuel filter (B).
4. Install the part in the reverse order of removal