## Design Specifications

####

2-8

Item | Measurement | Qualification | Specification
DIMENSIONS 3-door | Overall length |  | 4,140 mm (163.0 in.)
Overall width |  | 1,695 mm (66.7 in.)
Overall height | without roof antenna | 1,425 mm (56.1 in.)
with roof antenna | 1,550 mm (61.0 in.)
Wheelbase (MPW condition) |  | 2,570 mm (101.2 in.)
Track (MPW condition) | Front | 1,469 mm (57.8 in.)
Rear | 1,472 mm (58.0 in.)
Ground clearance |  | 129.7 mm (5.11 in.)
Seating capacity |  | Four (4)
DIMENSIONS 5-door | Overall length |  | 4,285 mm (168.7 in.)
Overall width |  | 1,695 mm (66.7 in.)
Overall height | without roof antenna | 1,495 mm (58.9 in.)
with roof antenna | 1,585 mm (62.4 in.)
Wheelbase |  | 2,685 mm (105.7 in.)
Track | Front | 1,472 mm (58.0 in.)
Rear | 1,489 mm (58.6 in.)
Ground clearance |  | 104 mm (4.10 in.)
Seating capacity |  | Five (5)
WEIGHT | Curb weight |  | 1,199 – 1,208 kg (2,643 – 2,663 lbs)
Max. permissible weight |  | 1,550 kg (3,417 lbs)
ENGINE | Type | 4EE2 | Water-cooled, Turbocharged, 4-stroke DOHC direct injection diesel engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke |  | 79 x 86 mm (3.11 x 3.39 in.)
Displacement |  | 1,686 cm3 (103 cu in.)
Compression ratio |  | 18.4
Valve train |  | Belt driven, DOHC 4 valves per cylinder
Lubrication system |  | Forced wet sump, with trochoid pump
Oil pump displacement | at 2,000 rpm (min-1) | 32.1 l (33.9 US qt, 28.2 Imp qt)/minute
Water pump displacement | at 5,200 rpm (min-1) | 185 l (195 US qt, 163 Imp qt)/minute
Fuel required |  | EC REF. Fuel
STARTER | Type |  | Gear reduction
Normal output |  | 1.4 kW
Hour rating |  | 30 seconds
Direction of rotation |  | Clockwise as viewed from gear end

a a a