## Exterior Lights

#### Taillight Replacement

22-26

Taillights:

1. Open the trunk lid.
2. Disconnect each connector from the taillight.

Brake/Taillight:21/5 W

Back-up Light18 W

Turn Signal Light:27 W

Side Marker Light

(KK, KX, KY):3.8 W

3. Remove the four nuts and taillight.
4. Install in the reverse order of removal.
5. When installing the taillight check the gasket; if it is distorted or stays compressed, replace it.
6. After installing the taillight run water over the taillight to make sure it does not leak.