## Doors

#### Rear Door Sash Trim Replacement

20-22

Rear Door Glass Outer Weatherstrip Replacement

NOTE: Take care not to scratch the door.

1. Pull back the door weatherstrip (A) at the front upper corner portion, and remove the screw.

   Fastener Location
   : Screw, 1

2. Pull up the door sash trim (B) to release the hooks (C), then remove the trim. Take care not to damage the door glass outer weatherstrip (D).
3. Install the reverse order of removal.

NOTE:

- Put on gloves to protect you hands.
- Take care not to scratch the door.

1. Starting at the front, pry the door glass outer weatherstrip (A) up to detach the clips (B, C, D), then remove the weatherstrip.

   Fastener Locations
   B : Clip, 1 | C : Clip, 3 | D : Clip, 1

2. Install the weatherstrip in the reverse order of removal, and replace any damaged clips.