## Fuel and Emissions Systems

#### System Descriptions (cont'd)

11-179

PCM Inputs and Outputs at Connector C (22P)

Wire side of female terminals

NOTE: Standard battery voltage is 12 V.

Terminal number | Wire colour | Terminal name | Description | Signal
11*18 | BLU | ATP2 (TRANSMISSION RANGE SWITCH 2 POSITION) | Detects transmission range switch 2 position signal | In 2nd position: about 0 V In any other position: about 5 V or battery voltage
11*16 | BLU | ATPL (TRANSMISSION RANGE SWITCH L POSITION) | Detects transmission range switch L signal | In L position: about 0 V In any other position: about 5 V or battery voltage
12*17 | BLU/WHT | ATPNP (TRANSMISSION RANGE SWITCH NEUTRAL/PARK POSITION) | Detects transmission range switch Neutral/Park position signal | In Park or Neutral: about 0 V In any other position: about 5 V or battery voltage
14*18 | GRN | NCSG (COUNTERSHAFT SPEED SENSOR GROUND) | Ground for countershaft speed sensor |
15*18 | BLU | NC (COUNTERSHAFT SPEED SENSOR) | Detects Countershaft speed sensor signal | With ignition switch ON (II), and front wheels rotating: battery voltage
15*16 | WHT/GRN | NDN (CVT DRIVEN PULLEY SPEED SENSOR) | Detects CVT driven pulley speed sensor signal | In other than Park or neutral: pulses
16*16 | GRN/YEL | SHLS - (CVT SPEED CHANGE CONTROL VALVE-SIDE) | Ground for CVT speed change control valve | With ignition switch ON (II): duty controlled
20*17 | YEL | ATPD (TRANSMISSION RANGE SWITCH D POSITION) | Detects transmission range switch D position signal | In D position: about 0 V In any other position: about 5 V or battery voltage
21*18 | WHT/GRN | NMSG (MAINSHAFT SPEED SENSOR GROUND) | Ground for mainshaft speed sensor |
22*16 | WHT/RED | VEL1 (CVT SPEED SENSOR 1) | Detects CVT speed sensor 1 | Depending on vehicle speed: pulses When vehicle is stopped: about 0 V

*1: with TWC model (except KV model) *2: without TWC model *3: D15Y4, D17A2 (KU, KQ, KZ, FO models) engines *4: with cruise control *5: D15Y4, D17A2 (KU model) engines

*6: D15Y4, D16W8, D16W9, D17A2, D17A5, D17Z3, D17Z4 engines

*7: D16W8, D16W9 engines

*8: except D15Y2, D15Y3, D15Y5, D15Y6 engines

*9: D15Y6 engine

*10: D15Y4, D17A2 (KU, KQ, KZ, FO models), D17Z1 (KQ model) engines

*11:KU model

*12 except KU model

*13: D15Y6, D15Y3 (KY model with immobiliser, KN model), D15Y5, D15Y4, D17Z1 (KQ, KZ models), D17A1 (KK model), D17A2 (except MA model), D17A5 (KY model with immobiliser, KN model) engines

*14: except D15Y3 (PA, KW, KT, KN models), D16W9 (PA model), D17A5 (KN model) engines

*15: A/T and M/T

*16: CVT

*17: A/T and CVT

*18: A/T

*19:except D15Y6, D15Y3 (KY model with immobiliser, KN model), D15Y5, D15Y4, D17Z1 (KQ, KZ models), D17A1 (KK model), D17A2 (except MA model), D17A5 (KY model with immobiliser, KN model) engine