## Honda Multi Matic Transmission/CVT

#### Transmission Removal (cont'd)

14-325

11. Remove the spring clip (A) and washers (B).

12. Remove the two bolts securing the shift cable bracket (C), then separate the shift cable (D) from the control lever (E). Do not bent the shift cable excessively.
13. Disconnect the transmission range switch connector (A), CVT driven speed sensor connector (B), CVT speed sensor connector (C) and vehicle speed sensor connector (D).

14. Remove the ATF cooler hoses (A) from the ATF cooler lines (B). Turn the ends of the ATF cooler hoses up to prevent ATF from flowing out, then plug the ATF cooler hoses and lines.

NOTE: Check for any signs of leakage at the hose joints.

15. Disconnect the primary HO2S connector (A) and remove its harness (B) from the clamps (C).