## Driveline/Axle

#### Driveshaft Reassembly (cont'd)

16-10

U.S. and Canada produced models:

1. INBOARD JOINT
2. CIRCLIP
3. (Right driveshaft)
4. ROLLER
5. DOUBLE LOOP BAND

   Replace.

   (Replacement parts only)

6. INBOARD BOOT

   Pack cavity with grease.

7. EAR CLAMP BAND

   Replace.

8. LOW PROFILE BAND

   Replace.

9. SPIDER
10. Pack cavity with grease.
11. SET RING

    Replace.

12. Left driveshaft
13. EAR CLAMP BAND

    Replace.

14. DRIVESHAFT
15. STOP RING

    Replace.

16. EAR CLAMP BANDS

    Replace.

17. OUTBOARD JOINT
18. Pack cavity with grease.
19. OUTBOARD BOOT
20. Right driveshaft

    (Except SOHC engine A/T models)

21. DYNAMIC DAMPER

    (Undirectional)