## End Cover/Intermediate Housing

#### Forward Clutch, Reverse Brake and Intermediate Housing Removal (cont'd)

14-363

Special Tools Required Reverse brake spring compressor, 07TAE-P4V0110 NOTE: Refer to the Exploded View as needed during the following procedure.

1. Remove the end cover (three; 6 mm bolts and 11; 8 mm bolts).
2. Remove the manual valve body lines A and B.
3. Remove the planetary carrier/input shaft assembly and ring gear.
4. Remove the snap ring securing the reverse brake discs and plates, then remove the reverse brake and plate, discs, plates and disc spring.
5. Remove the snap ring securing the forward clutch end plate, then remove the forward clutch end plate, discs and plates.
6. Remove the snap ring securing the forward clutch to the drive pulley shaft, then remove the forward clutch.
7. Install the special tool to remove the snap ring securing the reverse brake return spring retainer.

8. Compress the return spring with the special tool, then remove the snap ring. Be sure the special tool set over the reverse brake return springs.

9. Remove the special tool, then remove the spring retainer/return spring assembly (A).

10. Apply air pressure to reverse brake pressure circuit hole (B) to remove the reverse brake piston (C).
11. Remove the snap ring retainer from the drive pulley shaft.
12. Remove the manual valve body (five bolts) and separator plate.
13. Remove the roller and push the control shaft toward the outside of the transmission housing, then remove the intermediate housing (four bolts).