## Steering

#### Steering Linkage and Gearbox Inspection

17-5

NOTE: LHD type is shown, RHD type is symmetrical.

1. BOOTS

   Inspect for damage and deterioration.

2. STEERING COLUMN

   Inspect for loose column mounting nuts and bolts.

3. STEERING JOINTS

   Check for loose joint bolts.

4. TIE-ROD END BALL JOINT

   Inspect for faulty movement and damage.

5. BALL JOINT BOOT

   Inspect for damage and deterioration.

6. TIE-ROD LOCKNUTS

   Check for loose locknut.

7. STEERING GEARBOX

   Inspect for loose mounting nuts and bolts.

   GEARBOX MOUNTING CUSHIONS

   Inspect for deterioration.