## Honda Multi Matic Transmission/CVT Differential

#### Component Location Index

14-387

Backlash Inspection

1. FINAL DRIVEN GEAR

   Replacement, page 14-388

2. CARRIER BEARING

   Replacement, page 14-388

3. DIFFERENTIAL CARRIER

   Backlash Inspection, page 14-387

   Replacement, page 14-388

4. CARRIER BEARING

   Replacement, page 14-388

5. SET RING, 80 mm

   Selection, page 14-390

1. Place the differential assembly on V-blocks (A) and install both axles.

2. Check the backlash of the pinion gears (B) with a dial indicator (C).

   STANDARD: 0.05-0.15 mm (0.002-0.006 in.)

3. If the backlash is out of standard, replace the differential carrier.