## Standards and Service Limits

#### Fuel and Emissions

2-7

Item | Measurement | Qualification | Standard or New | Service Limit
Fuel pressure | Pressure with fuel pressure gauge connected |  | 270-320 kPa (2.8-3.3 kgf/cm2, 40-47 psi)
Fuel tank | Capacity |  | 45 l (11.9 US gal, 9.9 Imp gal)
Engine idle | Idle speed with headlights and radiator fan off | M/T in neutral | 700+50 rpm
A/T in or | 700+50 rpm
Fast idle | M/T in neutral | 1,250+50 rpm
A/T in or | 1,250+50 rpm
Idle CO% | Except D16V3 engine | 0.1 max.
D16V3 engine | 1.0 max.

Clutch

Item | Measurement | Qualification | Standard or New | Service Limit
Clutch pedal | Height | from the floor | 198 mm (7.8 in.) | -
Stroke |  | 130-140 mm (5.1-5.5 in.) | -
Play |  | 8-18 mm (0.3-0.7 in.) | -
Disengagement height | from the floor | 113 mm (4.4 in.) min. | -
Flywheel | Runout on clutch mating surface |  | 0.06 mm (0.002 in.) max. | 0.15 mm (0.006 in.)
Clutch disc | Rivet head depth |  | 1.2-1.7 mm (0.047-0.067 in.) | 0.2 mm (0.01 in.)
Thickness |  | 8.3-9.0 mm (0.33-0.35 in.) | 5.7 mm (0.22 in.)
Pressure plate | Warpage |  | 0.03 mm (0.001 in.) max. | 0.15 mm (0.006 in.)
Height of diaphragm spring fingers | Measure with feeler gauge and special tool | 0.6 mm (0.02 in.) max. | 1.0 mm (0.04 in.)