## Clutch

#### Clutch Master Cylinder Installation

12-5b

NOTE: Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.

1. Fit to the clutch master cylinder (A) a new O-ring (B) and a clutch master cylinder seal (C).

7. For the left-side steering vehicles, remove the clutch line (A) from the clutch line clip (B) (2 places).

8. Fit to the master cylinder (A) the reservoir hose (B), the clutch line (C) and a new retaining clip (D).

- For the left-side steering vehicle, it is not necessary to use the retaining clip holder that was removed when removing the clutch master cylinder.

9. To prevent the retaining clip (A) from coming off, pry open the tip of the retaining clip (B) with a screwdriver.

- For the left-side steering vehicles, pry it open from the inside of the left front wheelhouse with a screwdriver.

12-5a 12-5c home