## Air Conditioning

#### Compressor Replacement (cont'd)

21-88

9. Install the compressor in the reverse order of removal and note these items:

- If you are installing a new compressor, you must calculate the amount of refrigerant oil to be removed from it (see page 21-66).
- Replace the O-rings with new ones at each fitting and apply a thin coat of refrigerant oil before installing them. Be sure to use the right O-rings for HFC-134a (R-134a) to avoid leakage.
- Use refrigerant oil (SANDEN SP-10) for HFC-134a SANDEN spiral type compressor only.
- To avoid contamination, do not return the oil to the container once dispensed and never mix it with other refrigerant oils.
- Immediately after using the oil, reinstall the cap on the container and seal it to avoid moisture absorption.
- Do not spill the refrigerant oil on the vehicle; it may damage the paint; if the refrigerant oil contacts the paint, wash it off immediately.
- Be careful not to damage the radiator fins when installing the compressor and the condenser fan shroud.
- Charge the system (see page 21-96).
- Check for system performance (see page 20-98).
- Enter the anti-theft code for the radio, then enter the customer's radio station presets.