## Rear Side Outer Panel

#### Removal

3-7

- Cut and pry off the rear side outer panel.
- Check the rear pillar gutter lower and gutter upper position and check if for damage and if necessary, replace the rear pillar gutter lower.
- Check the centre pillar stiffener and check for damage. If necessary, replace the centre pillar stiffener lower.
- When replacing the centre pillar stiffener lower, remove the centre pillar separator and glue the insulator at the separator mounted position.

1. OUTER PANEL
2. CENTRE PILLAR STIFFENER LOWER
3. CENTRE PILLAR SEPARATOR
4. CENTRE PILLAR STIFFENER UPPER
5. REAR INNER PILLAR
6. REAR PILLAR GUTTER UPPER
7. REAR PANEL
8. REAR PILLAR GUTTER LOWER
9. REAR INNER PANEL
10. SIDE SILL REINFORCEMENT
11. REAR PILLAR GUTTER UPPER
12. REAR PILLAR GUTTER LOWER
13. REAR INNER PILLAR
14. REAR PANEL GUSSET
15. REAR PANEL
16. REAR GUTTER LOWERS STIFFENER
17. VIEW (Z)

a a a